For 1990-2009 cars

#### Special Tools

J 29714-A Servo Cover Depressor

For equivalent regional tools, refer to Special Tools.

1. Install the J 29714-A depressor .

Note: If cover does not move inwards with tool, use a block of wood or suitable material and lightly tap on cover using a hammer to free up cover in bore.

2. Tighten the J 29714-A depressor bolt to compress the servo cover.
3. Remove the servo cover retaining ring (29) and the J 29714-A depressor .
4. Remove the servo cover (28) and O-ring seal (27). If the servo cover seems to be hung up on the seal, cut and remove the O-ring seal before removing the cover.
5. Remove the 2-4 servo assembly.