For 1990-2009 cars

Scan Tool Output Control | Additional Menu Selection(s) | Description
--- | --- | ---
IPC Gages | -- | The IPC drives all gages to the maximum physical position when you select On. The IPC drives all gages to the minimum physical position when you select Off.
Lamp Test | -- | The IPC illuminates the following indicators when you select On:

• | ABS

• | Air Bag

• | Brake

• | CRUISE

• | Fasten safety belt

• | High beam

• | SECURITY

• | Upshift

The indicators should illuminate until commanded Off.

PRNDL Display | -- | An underscore illuminates under each indicator in the PRNDL display until commanded Off.
Segments Test | -- | All DIC and Odometer segments illuminate until commanded Off.