For 1990-2009 cars

## Steering Column Jacket Replacement Tilt Column

### Removal Procedure

1. Remove the steering column shaft. Refer to Steering Shaft Replacement.
2. Remove the steering column jacket bolts.
3. Remove the steering column jacket.

### Installation Procedure

1. Install the steering column jacket.

Caution: Refer to Fastener Caution in the Preface section.

2. Align and install the NEW steering column jacket bolts.

Tighten
Tighten the bolts to 17 N·m (13 lb ft).

3. Install the steering column shaft. Refer to Steering Shaft Replacement.