For 1990-2009 cars

### Removal Procedure

1. Remove the seat from the vehicle. Refer to Split Bench Seat Replacement or Front Seat Replacement - Bucket .
2. Remove the front seat back cover and pad. Refer to Front Seat Back Cushion Cover and Cushion Pad Replacement .
3. Remove the 2 hog ring fasteners (3) on the bottom of the seat back panel (2).
4. Remove the push-pin fastener (1) from the top of the seat back panel.
5. Remove the seat-back panel.

### Installation Procedure

1. Position the seat back panel on the seat-back frame.
2. Install the seat back panel to the frame with a push-pin fastener (1) at the top of the panel.
3. Install the 2 hog ring fasteners (3) to the bottom of the seat back panel (2).
4. Install the front seat back cover and pad. Refer to Front Seat Back Cushion Cover and Cushion Pad Replacement .
5. Install the seat in the vehicle. Refer to Split Bench Seat Replacement or Front Seat Replacement - Bucket .