For 1990-2009 cars

### Removal Procedure

1. Remove the balance shaft drive chain. Refer to Balance Chain Replacement .
2. Remove the balance shaft chain guide bolts.
3. Remove the balance shaft chain guide.

### Installation Procedure

1. Install the balance shaft chain guide.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the balance shaft chain guide bolts.

Tighten
Tighten the bolts to 10 N·m (89 lb in).

3. Install the balance shaft drive chain. Refer to Balance Chain Replacement .