For 1990-2009 cars

### Composite Headlamp System

1. Low-Beam Headlamp

2. High-Beam Headlamp

To replace the headlamp bulbs:

1. Open the hood. See Hood Release .
2. Reach in and access the bulb sockets from inside the engine compartment.
3. Turn the bulb socket counterclockwise and pull it straight out of the headlamp assembly.
4. Unplug the electrical connector from the old bulb by releasing the clips on the bulb socket.
5. Plug in the electrical connector to the new bulb.
6. Place the connector with the new bulb into the headlamp assembly and turn it clockwise until it is tight.

### Sealed Beam Headlamps

To replace the sealed headlamp bulbs, do the following:

1. Remove the four retainer screws and the retainer.
2. Pull the headlamp assembly toward you and unplug the electrical connector from it.
3. Remove the old headlamp bulb.
4. Plug the electrical connector into the new headlamp bulb.
5. Push the new bulb straight into the socket until it clicks.
6. Push the headlamp assembly straight into place.
7. Reinstall the retainer screws and the retainer.