For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Disconnect the brown engine wiring harness electrical connector (1) from the brown NEUTRAL switch electrical connector (6).
3. Disconnect the brown NEUTRAL switch electrical connector (2) from the bracket (3).
4. Remove the transfer case NEUTRAL switch (1) and gasket (4) from the transfer case.

### Installation Procedure

Notice: Refer to Component Fastener Tightening Notice in the Preface section.

1. Install the transfer case NEUTRAL switch (1) and gasket (4) into the transfer case.

Tighten
Tighten the neutral switch to 39 N·m (29 lb ft).

2. Connect the brown NEUTRAL switch electrical connector (2) to the bracket (3).
3. Connect the brown engine wiring harness electrical connector (1) to the brown NEUTRAL switch electrical connector (6).
4. Lower the vehicle.