For 1990-2009 cars

## Rear Bumper Replacement Canyon/Colorado

### Removal Procedure

1. Remove the license plate lamp harness.
2. Remove the bumper bracket to frame bolts.
3. Remove the bumper.
4. Remove the bracket to bumper bolts.

### Installation Procedure

1. Install the bumper brackets to the bumper.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the bumper bracket to bumper bolts.

Tighten
Tighten the bracket to bumper bolts to 160 N·m (118 lb ft).

3. Install the bumper to the vehicle.
4. Install the bumper bracket to frame bolts.

Tighten
Tighten the bumper to frame bolts to 160 N·m (118 lb ft).