For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you review the Steering Wheel and Column Description and Operation? | Go to Step 2 | Go to Steering Wheel and Column Description and Operation
2 | Verify that the key cannot be removed from the lock cylinder in the OFF position. Does the lock system operate normally? | System OK | Go to Step 3
3 | Inspect for incorrect, worn, or damaged key. Is the key incorrect, worn, or damaged? | Go to Step 5 | Go to Step 4
4 | Inspect for a faulty lock cylinder or release button. Is the lock cylinder or release button damaged? | Go to Step 6 | Go to Step 3
5 | Replace the key. Refer to Key and Lock Cylinder Coding . Did you complete the repair? | Go to Step 7 | --
6 | Replace the lock cylinder. Refer to Ignition Lock Cylinder Replacement . Did you complete the repair? | Go to Step 7 | --
7 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 3