For 1990-2009 cars

#### Tools Required

• | J 8092 Universal Driver Handle - 3/4 in - 10

• | J 34196-B Transmission Bushing Service Set

### Removal Procedure

Using J 34196-5 which is part of kit J 34196-B with J 8092 , remove the input sun gear front bushing (657) and rear bushing (659).

### Installation Procedure

1. Using J 34196-4 which is part of kit J 34196-B with J 8092 , install the input sun gear front bushing (657).
2. Using J 34196-6 which is part of kit J 34196-B with J 8092 , install the input sun gear rear bushing (659).