For 1990-2009 cars

### Removal Procedure

1. Open the instrument panel (I/P) storage compartment.
2. Remove the screws retaining the storage compartment handle assembly.
3. Remove the handle assembly from the vehicle.

### Installation Procedure

1. Install the handle assembly the storage compartment.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the screws retaining the handle assembly to the storage compartment.

Tighten
Tighten the screws to 3 N·m (27 lb in).

3. Ensure the handle assembly is working properly.