For 1990-2009 cars

### Removal Procedure

1. Remove the rear door window regulator. Refer to Rear Side Door Window Regulator Replacement .
2. Remove the bolts retaining the rear window regulator motor to the regulator bracket.
3. Remove the rear window regulator motor from the regulator.

### Installation Procedure

1. Install the rear window regulator motor to the regulator.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the bolts retaining the rear window regulator motor to the regulator bracket.

Tighten
Tighten the rear window regulator motor bolts to 4.5 N·m (40 lb in).

3. Install the rear door window regulator. Refer to Rear Side Door Window Regulator Replacement .