For 1990-2009 cars

#### Tools Required

J 9886-01 Door Handle Clip Remover

### Removal Procedure

1. Remove the window regulator handle from the door by inserting tool J 9886-01 between the handle and the white plastic washer to remove the retaining clip, if the vehicle is equipped with manual windows.
2. Remove the retaining screw from the door handle bezel.
3. Remove the 2 retaining screws from the armrest.
4. Disconnect the electrical harness from the power window switch, if equipped.
5. Gently pull the door panel away from the door.
6. Remove any fasteners from the door and reinsert them in the door panel before installing the panel on the door.

### Installation Procedure

1. Install the trim panel to the door, ensuring that all the retaining tabs are fully seated.
2. Connect the electrical harness to the power window switch, if equipped.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the 2 retaining screws in the switch plate.

Tighten
Tighten the rear door switch plate screws to 2 N·m (18 lb in).

4. Install the retaining screw in the door handle bezel.

Tighten
Tighten the rear door handle bezel screws to 2 N·m (18 lb in).

5. Install the window regulator handle from the door and insert the clip between the handle and the white plastic washer, if the vehicle is equipped with manual windows.