For 1990-2009 cars

## Front Door Opening Weatherstrip Replacement Regular, Crew

### Removal Procedure

1. Open the front door.
2. Remove the lower center pillar panel. Refer to Center Pillar Lower Trim Panel Replacement .
3. Remove the front door opening weatherstrip (2) from the door opening pinchweld flange (1).
4. Remove the front door opening weatherstrip from the vehicle.

### Installation Procedure

1. Position the front door opening weatherstrip to the pinchweld flange.
2. Starting at the upper rear corner, press the front door opening weatherstrip (2) onto the pinchweld flange (1) until it is fully seated.
3. Install the lower center pillar panel. Refer to Center Pillar Lower Trim Panel Replacement .
4. Pull the cord (3) on the front door opening weatherstrip ensuring the weatherstrip lip overlaps the interior trim panels and headliner.
5. Close the front door.

## Front Door Opening Weatherstrip Replacement Extended

### Removal Procedure

1. Open the front and rear door.
2. Remove the front door opening weatherstrip (1) from the opening pinchweld flange.
3. Remove the front door opening weatherstrip from the vehicle.

### Installation Procedure

1. Align the paint dot on the front door weatherstrip to the notch (2) in the upper rear corner of the pitchweld flange.
2. Starting at the notch (2) in the upper rear corner, press the front door opening weatherstrip (1) onto the pinchweld flange until it is fully seated.
3. Pull the cord (3) on the front door opening weatherstrip, ensuring the weatherstrip lip overlaps the interior trim panels and headliner.
4. Close the front door.