For 1990-2009 cars

### Removal Procedure

1. Remove the bolt cover (1) using a flat-bladed plastic tool.
2. Remove the windshield garnish molding bolt (3) securing the molding to the pillar.
3. Remove the windshield garnish molding by pulling the molding away from the pillar.

### Installation Procedure

1. Position the windshield garnish molding on the pillar.
2. Install the molding by firmly pressing the molding against the pillar to seat the fasteners (2).

Caution: Refer to Fastener Caution in the Preface section.

3. Install the windshield garnish molding bolt (3) and tighten to 9 N·m (79 lb in).
4. Install the bolt cover (1).