For 1990-2009 cars

#### Tools Required

J 39400-A Halogen Leak Detector

### Removal Procedure

1. Remove the radiator. Refer to Radiator Replacement .
2. Recover the refrigerant. Refer to Refrigerant Recovery and Recharging .
3. Remove the receiver dryer.
4. Remove the condenser inlet hose bolt.
5. Remove the condenser inlet hose.
6. Remove the condenser outlet hose bolt.
7. Remove the condenser outlet hose.
8. Remove the condenser from mounts on the radiator (1).
9. Remove the condenser.

### Installation Procedure

Important: If replacing the condenser, add the refrigerant oil to the condenser. Refer to Refrigerant System Capacities for the capacity information.

1. Install the condenser to the radiator.
2. If replacing the condenser, transfer the components from the old condenser as necessary.
3. Install the condenser to the mounts on the radiator (1).

Notice: Refer to Fastener Notice in the Preface section.

4. Install the condenser retaining bolts to the radiator.

Tighten
Tighten the bolts to 28 N·m (21 lb ft).

5. Install the receiver dyer.
6. Install the condenser inlet hose.
7. Install the condenser inlet hose bolt.

Tighten
Tighten the bolts to 20 N·m (15 lb ft).

8. Install the condenser outlet hose.
9. Install the condenser outlet hose bolt.

Tighten
Tighten the bolts to 20 N·m (15 lb ft).

10. Install the radiator. Refer to Radiator Replacement .
11. Evacuate and recharge the A/C system. Refer to Refrigerant Recovery and Recharging .
12. Leak test the fittings of the components using the J 39400-A .