For 1990-2009 cars

#### Special Tools

J 21368 Pump Body and Cover Alignment Band

1. Place the oil pump cover onto the oil pump body and put stator shaft through a hole in the bench.
2. Install the pump cover bolts (233) finger tight only.
3. Install the J 21368 alignment band .

Caution: Refer to Fastener Caution in the Preface section.

4. Tighten the pump cover bolts (233). Tighten the bolts to 24 N·m (18 lb ft).
5. Remove the J 21368 alignment band .