For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear bumper impact bar brace. Refer to Rear Bumper Impact Bar Brace Replacement.

1 | Rear Bumper Impact Bar Bracket Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 100 N·m (74 lb ft)
2 | Rear Bumper Impact Bar Bracket Bolt (Qty: 2) Tighten 40 N·m (30 lb ft)
3 | Rear Bumper Impact Bar Bracket