For 1990-2009 cars

### Diagnostic Instructions

• | Perform the Diagnostic System Check - Vehicle prior to using this diagnostic procedure.

• | Review Strategy Based Diagnosis for an overview of the diagnostic approach.

• | Diagnostic Procedure Instructions provide an overview of each diagnostic category.

### Circuit/System Description

The body control module (BCM) sends a serial data message to the instrument panel cluster (IPC) requesting low tire pressure indicator illumination.

### Conditions for Running the DTC

Important: It is recommend that Component Testing is performed before Circuit Testing when diagnosing.

1. With the scan tool, select instrument panel special functions Lamp Test. Command the instrument panel warning lamps OFF.

⇒ | If the tire pressure monitor (TPM) warning lamp does not turn OFF, replace the IPC.

2. With the TPM special tool, transmit simulated tire pressures to the BCM. Observe the tire pressures in the scan tool data display.

⇒ | If the TPM simulated tire pressure is not within ±4 psi of the scan tool reading, replace the BCM.

### Component Testing

1. Inspect the tires for proper inflation pressure.

⇒ | Inflate tires to the proper pressure. Refer to Vehicle Certification, Tire Placard, Anti-Theft, and Service Parts ID Label .

2. Using the TPM special tool, activate each tire pressure sensor and record each sensors tire pressure reading in psi. Check tire pressures with a known accurate hand held tire pressure gauge and compare the psi reading to the display on the TPM special tool.

⇒ | If the TPM special tool displays a difference of 4 psi or more lower than actual tire pressure, replace the suspect tire pressure sensor.

⇒ | If actual and displayed tire pressure readings are normal, go to Circuit/System Testing.

### Repair Instructions

Perform the Diagnostic Repair Verification after completing the diagnostic procedure.

• | Tire Pressure Sensor Learn

• | Control Module References for BCM replacement, setup, and programming