For 1990-2009 cars

### Removal Procedure

Caution: Refer to Fuel and Evaporative Emission Pipe Caution in the Preface section.

Caution: Refer to Gasoline/Gasoline Vapors Caution in the Preface section.

Notice: Refer to Fuel and Evaporative Emission Hose/Pipe Connection Cleaning Notice in the Preface section.

1. Refer to Plastic Collar Quick Connect Fitting Service in order to disconnect the evaporative emission (EVAP) hose from the following:

• | The throttle body assembly (2)

• | The EVAP canister purge solenoid valve (3)

2. Remove the EVAP hose (1) from the engine.

### Installation Procedure

1. Position the EVAP hose (1) to the engine.
2. Refer to Plastic Collar Quick Connect Fitting Service in order to connect the EVAP hose to the following:

• | The throttle body assembly (2)

• | The EVAP canister purge solenoid valve (3)