For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Anchor Torsion Bar to Lower Control Arm Bolts | 80 N·m | 59 lb ft
Ball Joint to Control Arm Nuts - Lower 2WD | 60 N·m | 44 lb ft
Ball Joint to Control Arm Nuts - Lower 4WD and 2WD Z71 | 64 N·m | 47 lb ft
Ball Joint to Control Arm Nuts - Upper 2WD | 16 N·m | 12 lb ft
Ball Joint to Control Arm Nuts - Upper 4WD and 2WD Z71 | 47 N·m | 35 lb ft
Front Brake Rotor to Front Wheel Hub Bolt

- Initial Torque

20 N·m

15 lb ft

- Final Torque

110 N·m

81 lb ft

Hub and Bearing Assembly to Steering Knuckle Bolts | 110 N·m | 81 lb ft
Lower Control Arm Ball Joint Stud Nut | 138 N·m | 102 lb ft
Lower Control Arm to Frame Bolts Front - 4WD | 165 N·m | 122 lb ft
Lower Control Arm to Frame Bolts Rear - 4WD | 180 N·m | 133 lb ft
Lower Control Arm to Frame Nuts - 2WD | 155 N·m | 114 lb ft
Shock Absorber Tenon Nut - 2WD | 20 N·m | 15 lb ft
Shock Absorber Tenon Nut - 4WD | 24 N·m | 18 lb ft
Shock Absorber to Lower Control Arm Nut - 4WD | 70 N·m | 52 lb ft
Shock Absorber to Lower Control Arm Nut - 2WD | 110 N·m | 81 lb ft
Spring/Shock Assembly to Frame Nuts | 27 N·m | 20 lb ft
Stabilizer Shaft Insulator Clamp Bolts | 50 N·m | 37 lb ft
Stabilizer Shaft Link Nuts | 44 N·m | 32 lb ft
Upper Control Arm Ball Joint Stud Nut | 100 N·m | 74 lb ft
Upper Control Arm to Frame Bolts - 2WD | 160 N·m | 118 lb ft
Upper Control Arm to Frame Nuts - 4WD and 2WD Z71 | 155 N·m | 114 lb ft
Wheel Speed Sensor Mounting Bracket Bolt | 20 N·m | 15 lb ft