For 1990-2009 cars

## Transfer Case Adapter Replacement M30

### Removal Procedure

1. Remove the transfer case assembly. Refer to Transfer Case Assembly Replacement .

Important: The transmission mount DOES NOT have to be removed to perform the following service procedure.

2. Remove the 2 transmission mount bolts.
3. Position a transmission jack under the transmission.
4. Lift the transmission just high enough to remove the transfer case adapter.
5. Remove the transfer case adapter mounting bolts.
6. Remove the transfer case adapter from the transmission.
7. Remove the transfer case adapter seal.

### Installation Procedure

1. Lightly lubricate the transfer case adapter seal with clean transmission fluid.
2. Position the NEW seal to the transfer case adapter.
3. Install the transfer adapter to the transmission.

Notice: Refer to Fastener Notice in the Preface section.

4. Install the transfer case adapter mounting bolts to the transmission.

Tighten
Tighten the transfer case adapter mounting bolts to 50 N·m (37 lb ft).

5. Lower the transmission to the transmission mount.
6. Install the transmission mount bolts.

Tighten
Tighten the transmission mount bolts to 50 N·m (37 lb ft).

7. Remove the transmission jack.
8. Install the transfer case assembly. Refer to Transfer Case Assembly Replacement .