For 1990-2009 cars

### Removal Procedure

1. Remove the seat from the vehicle. Refer to Front Seat Replacement - Bucket .
2. Remove the seat back cover to expose the heater element. Refer to Front Seat Back Cushion Cover and Cushion Pad Replacement .
3. Disconnect the electrical harness from the heater element.
4. Remove the heater element (1) by peeling the element off the pad (2).
5. Pull the heater element electrical harness through the hole (3) in the pad.

### Installation Procedure

1. Install the heater element electrical harness through the hole (3) in the pad.
2. Install the adhesive-backed heater element (1) to the pad (2) by pressing in place.
3. Connect the electrical harness to the heater element.
4. Install the seat back cover. Refer to Front Seat Back Cushion Cover and Cushion Pad Replacement .
5. Install the seat in the vehicle. Refer to Front Seat Replacement - Bucket .