For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.

1 | Camshaft Position Sensor Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Clean the area around the camshaft position (CMP) sensor before removal in order to prevent debris from entering the engine.

Tighten
12 N·m(106 lb in)

2 | Camshaft Position Sensor Bracket Assembly

#### Procedure

Disconnect the electrical connectors.

3 | Camshaft Position Sensor
4 | Camshaft Position Sensor O-ring Seal

#### Procedure

Lubricate the O-ring seal with clean engine oil.