For 1990-2009 cars

#### Tools Required

J 3049-A Valve Lifter Remover

### Removal Procedure

1. Remove the cylinder head and gasket. Refer to Cylinder Head Replacement - Left Side or to Cylinder Head Replacement - Right Side.
2. Remove the valve lifter. Refer to Valve Lifter Removal.
3. Clean and inspect the valve lifters. Refer to Valve Lifter and Guide Cleaning and Inspection.

### Installation Procedure

1. Install the valve lifter. Refer to Valve Lifter Installation.
2. Install the cylinder head and gasket. Refer to Cylinder Head Replacement - Left Side or to Cylinder Head Replacement - Right Side.