For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Open the sunshade to the full open position.
2. Remove the sunroof front trim cover. Refer to Sunroof Front Trim Cover Replacement .

1 | Sunroof Motor Screw (Qty: 2) Notice: Refer to Fastener Notice in the Preface section.

#### Procedure

Disconnect the electrical connector.

Tighten
3 N·m (27 lb in)

2 | Sunroof Motor

#### Procedure

Rock the motor back and forth to release it from the cables.

Tip

• | When installing the motor spline into the gear, Do not twist the sunroof motor from side to side as it is aligned. If twisted, this may cause the cables to misalignment and the window panel will not close evenly on both side.

• | After install motor verify sunroof track timing/synchronization. Refer to Sunroof Track Timing/Synchronization .

• | Verify operations of the sunroof window.