For 1990-2009 cars

## Front Fog Lamp Bulb Replacement Canyon

### Removal Procedure

1. Turn the fog lamp switch to the OFF position.
2. Disconnect the electrical connector.
3. Rotate the bulb socket counterclockwise in order to release the socket from the fog lamp housing.
4. Remove the socket from the fog lamp housing.
5. Remove the bulb from the socket (2).

### Installation Procedure

1. Install the bulb to the socket (2).
2. Index the tabs on the bulb socket to the slots in the fog lamp housing.
3. Install the socket to the fog lamp housing.
4. Rotate the socket clockwise until fully seated.