For 1990-2009 cars

### Removal Procedure

1. Position the front door window approximately halfway down.
2. Remove the front door trim panel. Refer to Front Side Door Trim Panel Replacement .
3. Remove the front door water deflector. Refer to Front Side Door Water Deflector Replacement .
4. Remove the front door outer belt sealing strip. Refer to Front Side Door Window Belt Outer Sealing Strip Replacement .
5. Remove the bolts retaining the front door window to the window regulator.
6. Lift the window off of the window regulator.
7. Rotate the rear of the window upwards, disengaging the window from the window run channel.
8. Remove the window from between the inner and outer door panels.

### Installation Procedure

1. Install the front door window into the front door between the inner and outer door panels.
2. Rotate the rear of the window down, positioning the window into the window run channels.
3. Lower the window down onto the window regulator.

Notice: Refer to Fastener Notice in the Preface section.

4. Install the bolts retaining the front door window to the window regulator.

Tighten
Tighten the front window bolts to 9 N·m (80 lb in).

5. Install the front door outer belt sealing strip. Refer to Front Side Door Window Belt Outer Sealing Strip Replacement .
6. Install the front door water deflector. Refer to Front Side Door Water Deflector Replacement .
7. Install the front door trim panel. Refer to Front Side Door Trim Panel Replacement .