For 1990-2009 cars

## Rear Seat Cushion Cover and Pad Replacement Extended Cab

### Removal Procedure

1. Remove the rear folding seat cushion from the vehicle. Refer to Folding Seat Replacement .
2. Release the J-strips (2) on the cover (1).
3. Remove the seat cushion cover from the seat frame/pad.

### Installation Procedure

1. Install the seat cushion cover over the seat frame/pad.
2. Install the J-strips (2) on the cover (1).
3. Install the rear folding seat cushion in the vehicle. Refer to Folding Seat Replacement .

## Rear Seat Cushion Cover and Pad Replacement Crew Cab

### Removal Procedure

1. Remove the rear bench seat from the vehicle. Refer to Rear Bench Seat Replacement .
2. Remove the seat belt buckles (1) from the seat cover loops (2).
3. Release the J-strips (1) on the cover.
4. Remove the seat cushion cover and pad from the seat frame (2).

### Installation Procedure

1. Install the seat cushion cover and pad over the seat frame (2).
2. Install the J-strips (1) on the cover.
3. Install the seat belt buckles (1) through the seat cover loops (2).
4. Install the rear bench seat in the vehicle. Refer to Rear Bench Seat Replacement .