For 1990-2009 cars

### Removal Procedure

1. Open the rear side access door.
2. Remove the rear side access upper door striker trim cover. Refer to Rear Side Door Latch Striker Cover Replacement .
3. Remove the bolts retaining the upper side access door striker to the body.
4. Remove the upper side access door striker from the body.

### Installation Procedure

1. Install the upper side access door striker to the body.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the bolts retaining the upper side access door striker to the body.

Tighten
Tighten the upper side access door striker bolts to 25 N·m (18 lb ft).

3. Install the rear side access upper door striker trim cover. Refer to Rear Side Door Latch Striker Cover Replacement .
4. Close the rear side access door.