For 1990-2009 cars

### Removal Procedure

1. Remove the front seat assembly from the vehicle. Refer to Front Seat Replacement - Bucket or Split Bench Seat Replacement .
2. Remove the front seat cushion cover and pad. Refer to Front Seat Cushion Cover and Pad Replacement .
3. Disconnect the electrical harness from the heater element.
4. Remove the heater element (1) by peeling the element off the pad (2).
5. Pull the heater element electrical harness through the hole (3) in the pad.

### Installation Procedure

1. Install the heater element electrical harness through the hole (3) in the pad.
2. Install the adhesive-backed heater element (1) to the pad (2) by pressing in place.
3. Connect the electrical harness to the heater element.
4. Install the front seat cushion cover and pad. Refer to Front Seat Cushion Cover and Pad Replacement .
5. Install the front seat assembly in the vehicle. Refer to Front Seat Replacement - Bucket or Split Bench Seat Replacement .