For 1990-2009 cars

### Removal Procedure

1. Remove the accessory drive belt. Refer to Drive Belt Replacement - Accessory.
2. Remove the cooling fan. Refer to Fan Replacement.
3. Cut the belt (1) from air conditioning (A/C) and crankshaft pulleys.

### Installation Procedure

1. Position the belt behind the rear face of the balancer (1) and off of the A/C pulley (2).
2. Install the belt installation tool (3) onto the balancer.
3. Slide the belt installation tool (1) upward, installing the belt (2) onto the belt installation tool.
4. Slide the belt installation tool downward, positioning the belt onto the A/C pulley, applying light tension to the belt.
5. Position the lower portion of the belt (1) with the ribbed area facing forward.
6. Slowly rotate the crankshaft pulley (1) in a clockwise direction while using finger pressure to pull the belt (2) forward. Ensure that the ribbed area of the belt remains facing forward and the belt aligns properly to the A/C pulley.
7. Inspect the drive belt (1) for proper installation and alignment.
8. Rotate the balancer (1) and additional 360 degrees to ensure proper belt installation.
9. Install the cooling fan. Refer to Fan Replacement.
10. Install the accessory drive belt. Refer to Drive Belt Replacement - Accessory.