For 1990-2009 cars

### Removal Procedure

1. Open the rear seat belt upper guide shoulder bolt trim cover.
2. Remove the rear seat belt upper guide shoulder bolt.
3. Remove the body rear corner trim panel. Refer to Body Side Rear Lower Trim Panel Replacement.
4. Remove the rear seat belt anchor bolt.
5. Remove the bolt that retains the seat belt retractor assembly to the body.
6. Remove the rear seat belt assembly from the vehicle.

### Installation Procedure

1. Position the rear seat belt retractor assembly to the vehicle.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the bolt which retains the seat belt retractor assembly to the body.

Tighten
Tighten the rear seat belt retractor bolt to 52.5 N·m (39 lb ft).

3. Install the rear seat belt upper guide with the bolt. Ensure that the seat belt webbing is not twisted.

Tighten
Tighten the rear seat belt upper guide bolt to 52.5 N·m (39 lb ft).

4. Install the rear seat belt upper guide shoulder bolt trim cover.
5. Install the body rear corner trim panel. Refer to Body Side Rear Lower Trim Panel Replacement.
6. Install the rear seat belt anchor bolt. Ensure that the seat belt webbing is not twisted.

Tighten
Tighten the rear seat belt anchor bolt to 52.5 N·m (39 lb ft).