For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the oil pressure test plug.

### Installation Procedure

Notice: Refer to Component Fastener Tightening Notice in the Preface section.

1. Install an oil pressure test plug.

Tighten
Tighten the oil pressure test plug to 8 N·m (71 lb in).

2. Check the transmission fluid level, fill if necessary. Refer to Transmission Fluid Check .
3. Lower the vehicle.