For 1990-2009 cars

### Removal Procedure

1. Remove the accessory drive belt. Refer to Drive Belt Replacement - Accessory.
2. Remove the drive belt tensioner bolts.
3. Remove the drive belt tensioner.

### Installation Procedure

1. Position the drive belt tensioner to the water pump.

Caution: Refer to Fastener Caution in the Preface section.

2. Install and tighten the drive belt tensioner bolts.

Tighten
Tighten the bolts to 50 N·m (37 lb ft).

3. Install the accessory drive belt. Refer to Drive Belt Replacement - Accessory.