For 1990-2009 cars

# Driver Information and Entertainment

## All Component Locator

- Displays and Gages Component Views

## All Description and Operation

- Audible Warnings Description and Operation
- Compass Calibration and Magnetic Variance
- Door Ajar Indicator Description and Operation
- Driver Information Center (DIC) Description and Operation
- Indicator/Warning Message Description and Operation
- Instrument Cluster Description and Operation

## All Visual Identification

- Displays and Gages Connector End Views

## Diagnostic Procedures

- Chime Always On
- Chime Inoperative
- Diagnostic Starting Point - Displays and Gages
- Door Ajar Indicator Malfunction
- Engine Coolant Temperature Gage Inaccurate or Inoperative
- Engine Oil Pressure Indicator Always On
- Fuel Gage Inaccurate or Inoperative
- Mirror Compass Display Inoperative or Inaccurate
- Mirrors - Temperature Display Inaccurate
- Mirrors - Temperature Displays SC or OC
- Odometer Trip/Reset Switch Inoperative
- Speedometer and/or Odometer Inaccurate or Inoperative
- Symptoms - Displays and Gages
- Tachometer Inaccurate or Inoperative

## Diagnostic Trouble Codes

- DTC P0461
- DTC P0462
- DTC P0463
- DTC P0464
- DTC P0520

## Electrical/Electronic Schematic Diagrams

- Audible Warnings Schematics
- Instrument Cluster Schematics

## Electrical/Electronic Specifications

- Fuel Level Specifications

## General Diagnostic Information

- Scan Tool Data Definitions
- Scan Tool Data List
- Scan Tool Output Controls

## Mechanical Specifications

- Fastener Tightening Specifications

## Removal, Installation, and Replacement

- Accessory Switch Replacement
- Ambient Air Temperature Sensor Replacement
- Instrument Cluster Lens Replacement
- Instrument Cluster Replacement