For 1990-2009 cars

### Removal Procedure

1. Loosen the air cleaner outlet duct clamps.
2. Remove the air cleaner outlet duct (1) from the following:

• | The air cleaner assembly

• | The air cleaner resonator

### Installation Procedure

Important: Ensure the notches (2) on the air cleaner outlet duct (1) are aligned with the following:

• | The air cleaner assembly tang (4)

• | The air cleaner resonator tang (3)

1. Install the air cleaner outlet duct to the following:

• | The air cleaner assembly

• | The air cleaner resonator

Notice: Refer to Fastener Notice in the Preface section.

2. Tighten the air cleaner outlet duct clamps.

Tighten
Tighten the air cleaner outlet duct clamps to 6 N·m (53 lb in).