For 1990-2009 cars

### Removal Procedure

1. Remove the HVAC module assembly. Refer to HVAC Module Assembly Replacement.
2. Remove the recirculation actuator screws.
3. Remove the electrical connector (3) from the recirculation actuator (2).
4. Remove the recirculation actuator.

### Installation Procedure

1. Install the recirculation actuator (2).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the screws to the recirculation actuator. Tighten the screws to 1.9 N·m (17 lb ft).
3. Connect the electrical connector (3) to the recirculation actuator (2).
4. Install the HVAC module assembly. Refer to HVAC Module Assembly Replacement.