For 1990-2009 cars

Important:

• | When replacing the worn or cracked bearings and the cups, replace the bearings in sets.

• | The low mileage bearings may have very small scratches and pits on the rollers and the bearing cups from the initial preload.

| Do not replace a bearing for this reason.

1. Inspect the bearings for smooth rotation after oiling.
2. Inspect the bearing rollers for wear.
3. Inspect the bearing cups for the following conditions:

• | Wear

• | Cracks

• | Brinelling

• | Scoring