For 1990-2009 cars

### Removal Procedure

1. Remove the grille. Refer to Grille Replacement.
2. Place the grille on a clean, prepared surface.
3. Remove the emblem retaining nuts.
4. Remove the emblem from the grille.

### Installation Procedure

1. Install the emblem to the grille.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the nuts that retain the emblem to the grille.

Tighten
Tighten the nuts to 3 N·m (27 lb in).

3. Install the grille. Refer to Grille Replacement.