For 1990-2009 cars

### Removal Procedure

1. Open the tailgate.
2. Remove the screws (1) from the tail lamp assembly.
3. Remove the lamp assembly.
4. Remove the tail lamp sockets by depressing the locking tab and rotating counterclockwise.
5. Remove the bulbs from the tail lamp and/or side marker lamp sockets.

### Installation Procedure

1. Install the bulbs to the tail lamp, and/or side marker lamp sockets.
2. Install the tail lamp sockets to the tail lamp, rotating clockwise until the locking tab is fully seated.
3. Press the tail lamp to the rear body panel until fully seated.

Caution: Refer to Fastener Caution in the Preface section.

4. Install the tail lamp screws (1) to the tail lamp.

Tighten
Tighten the tail lamp screws (1) to 3 N·m (26 lb in).

5. Close the tailgate.