For 1990-2009 cars

#### Tools Required

• | J 36850 Transjel Lubricant

• | J 44339 Reverse Synchronizer Installer

1. Install a new input shaft bearing on the input shaft. The bearing retaining ring groove goes forward.
2. Using a hydraulic press and J 44339 , install the input shaft bearing in position.

Important: The retaining ring is a select fit. Always install a new retaining ring.

3. Select the maximum thickness retaining ring for the input shaft bearing, that will fit in the groove. Refer to Input Shaft Bearing Retaining Ring Specifications .
4. Install the input shaft bearing retaining ring.
5. Install the output front support bearing into the input shaft.
6. Fill the bearing with J 36850 .
7. Install the 4th gear blocking ring onto the input shaft.