For 1990-2009 cars

## Front Bumper Fascia Replacement Canyon/Colorado

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the front bumper (1) assembly. Refer to Front Bumper Replacement .
3. Remove the push-pins retaining the fascia (2) to the front bumper.
4. Pull the fascia straight forward to remove.

### Installation Procedure

1. Install the fascia (2) to the front bumper.
2. Install the push-pins retaining the fascia to the front bumper.
3. Install the front bumper (1) assembly. Refer to Front Bumper Replacement .
4. Lower the vehicle.