For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Open the end gate in order to remove the end gate liner assembly.

1 | Pick Up Box End Gate Liner Bolt (Qty: 9) Caution: Refer to Fastener Caution in the Preface section. Tighten 7 N·m (62 lb in)
2 | Pick Up Box End Gate Liner Tip Pull the top endgate liner edge from under the end gate upper finish molding end cap.