For 1990-2009 cars

## Front Side Door Emblem/Nameplate Replacement Canyon

#### Tools Required

J 25070 Heat Gun

### Removal Procedure

Important: Use the tape for protection and alignment marks for alignment of the new emblem.

1. Apply tape to the area around the door emblem.
2. Heat the emblem/nameplate, using a J 25070 ,152 mm (6 in) from the surface.
3. Apply the heat using a circular motion for about 30 seconds.

Notice: Use a plastic, flat-bladed tool to prevent paint damage when removing an emblem/name plate.

4. Remove the emblem/nameplate from the door surface using a plastic, flat-bladed tool.
5. Remove all adhesive from the door panel surface and the back of the emblem/nameplate using 3M™ scotch brite molding adhesive remover disk 3M™ P/N 07501 or equivalent.
6. Clean the door surface using varnish makers and painters (VMP) naphtha.

### Installation Procedure

1. If the location of the emblem/nameplate has not been marked, apply tape and use the following dimensions:

• | Dimension (a) is 251 mm (9.88 in) from the bottom of the door to the emblem/nameplate.

• | Dimension (b) is 157 mm (6.18 in) from the front of the door to the front of the emblem/nameplate.

2. Warm the door surface with a J 25070 ,152 mm (6 in) from the surface to a minimum of 21°C (70°F).

Important: Do not touch the adhesive backing of the emblem/nameplate.

3. Remove the backing from the front end of the emblem/nameplate.
4. Press the emblem/nameplate to the door panel surface while continuing to remove the backing.
5. Hand roll the emblem/nameplate to the door panel to ensure proper adhesion.
6. Inspect the emblem/nameplate for bonding.
7. Remove the tape from the area around the door emblem.

## Front Side Door Emblem/Nameplate Replacement Colorado

#### Tools Required

J 25070 Heat Gun

### Removal Procedure

Important: Use the tape for protection and alignment marks for alignment of the new emblem.

1. Apply tape to the area around the door emblem.
2. Heat the emblem/nameplate, using a J 25070 , 152 mm (6 in) from the surface.
3. Apply the heat using a circular motion for about 30 seconds.

Notice: Use a plastic, flat-bladed tool to prevent paint damage when removing an emblem/name plate.

4. Remove the emblem/nameplate from the door surface using a plastic, flat-bladed tool.
5. Remove all adhesive from the door panel surface and the back of the emblem/nameplate using 3M™ scotch brite molding adhesive remover disk 3M™ P/N 07501 or equivalent.
6. Clean the door surface using varnish makers and painters (VMP) naphtha.

### Installation Procedure

1. If the location of the emblem/nameplate has not been marked, apply tape and use the following dimensions:

• | Dimension (a) is 166 mm (6.54 in) from the bottom of the door to the emblem/nameplate.

• | Dimension (b) is 117.4 mm (4.62 in) from the front of the door to the front of the emblem/nameplate.

2. Warm the door surface with a J 25070 , 152 mm (6 in) from the surface to a minimum of 21°C (70°F).

Important: Do not touch the adhesive backing of the emblem/nameplate.

3. Remove the backing from the front end of the emblem/nameplate.
4. Press the emblem/nameplate to the door panel surface while continuing to remove the backing.
5. Hand roll the emblem/nameplate to the door panel to ensure proper adhesion.
6. Inspect the emblem/nameplate for bonding.
7. Remove the tape from the area around the door emblem.

## Front Side Door Emblem/Nameplate Replacement XTREME

#### Tools Required

J 25070 Heat Gun

### Removal Procedure

Important: Use the tape for protection and alignment marks for alignment of the new emblem.

1. Apply tape to the area around the door emblem.
2. Heat the emblem/nameplate, using a J 25070 , 152 mm (6 in) from the surface.
3. Apply the heat using a circular motion for about 30 seconds.

Notice: Use a plastic, flat-bladed tool to prevent paint damage when removing an emblem/name plate.

4. Remove the emblem/nameplate from the door surface using a plastic, flat-bladed tool.
5. Remove all adhesive from the door panel surface and the back of the emblem/nameplate using 3M™ scotch brite molding adhesive remover disk 3M™ P/N 07501 or equivalent.
6. Clean the door surface using varnish makers and painters (VMP) naphtha.

### Installation Procedure

1. If the location of the emblem/nameplate has not been marked, apply tape and use the following dimensions:

• | Dimension (a) is 145.0 mm (5.70 in) from the front of the door to the emblem/nameplate.

• | Dimension (b) is 165.0 mm (6.50 in) from the bottom of the door to the front of the emblem/nameplate.

• | Dimension (c) is 28.0 mm (1.11 in) from the feature line of the door to the front of the emblem/nameplate.

2. Warm the door surface with a J 25070 , 152 mm (6 in) from the surface to a minimum of 21°C (70°F).

Important: Do not touch the adhesive backing of the emblem/nameplate.

3. Remove the backing from the front end of the emblem/nameplate.
4. Press the emblem/nameplate to the door panel surface while continuing to remove the backing.
5. Hand roll the emblem/nameplate to the door panel to ensure proper adhesion.
6. Inspect the emblem/nameplate for bonding.
7. Remove the tape from the area around the door emblem.