For 1990-2009 cars

### Circuit Description

The intake camshaft position (CMP) sensor produces a 1X signal for each revolution of the intake camshaft. This signal is used for startability. If the PCM does not receive a crankshaft position (CKP) sensor signal, the engine should still start based off of the information from the CMP. The CMP is connected directly to the powertrain control module (PCM) and consists of the following circuits:

• | A 12-volt reference circuit

• | A low reference circuit

• | A CMP sensor signal circuit

If the PCM does not receive a CMP sensor pulse, DTC P0340 will set.

### DTC Descriptor

This diagnostic procedure supports the following DTC:

DTC P0340 Intake CMP Sensor Circuit

### Conditions for Running the DTC

• | The engine is running.

• | DTC P0340 runs continuously when the engine is running.

### Conditions for Setting the DTC

The PCM does not receive one CAM pulse within 3 seconds.

### Action Taken When the DTC Sets

• | The malfunction indicator lamp (MIL) will illuminate after two consecutive ignition cycles in which the diagnostic runs with the fault active.

• | The PCM records the operating conditions at the time when the diagnostic fails. This information stores in the Freeze Frame and Failure Records buffers.

• | A history DTC stores.

### Conditions for Clearing the MIL/DTC

• | The MIL will turn OFF after three consecutive ignition cycles in which the diagnostic runs without a fault.

• | A history DTC will clear after 40 consecutive warm-up cycles without a fault.

• | Clear the DTCs with a scan tool.

### Diagnostic Aids

• | The following conditions may cause this DTC to set:

- | Damage to the camshaft reluctor wheel

- | Damage to the CMP sensor

- | The sensor coming in contact with the reluctor wheel

- | Foreign material passing between the sensor and the reluctor wheel

• | If the condition is intermittent, refer to Intermittent Conditions .

### Test Description

The number below refers to the step number on the diagnostic table.

1. This step tests the output of the CMP sensor. If the duty cycle is not within the specified range the sensor is bad.

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
Schematic Reference: Engine Controls Schematics Connector End View Reference: Powertrain Control Module Connector End Views or Engine Controls Connector End Views
1 | Did you perform the Diagnostic System Check - Vehicle? | -- | Go to Step 2 | Go to Diagnostic System Check - Vehicle
2 | Attempt to start the engine. Does the engine start and run? | -- | Go to Step 3 | Go to Step 7
3 |

1. Observe the Freeze Frame/Failure Records for this DTC.
2. Turn OFF the ignition for 30 seconds.
3. Start the engine.
4. Operate the vehicle within the Conditions for Running the DTC. You may also operate the vehicle within the conditions that you observed from the Freeze Frame/Failure Records.

Did the DTC fail this ignition?

--

Go to Step 4

Go to Diagnostic Aids

4 |

1. Turn OFF the ignition.
2. Disconnect the camshaft position (CMP) sensor.
3. Turn ON the ignition, with the engine OFF.
4. Probe the 12-volt reference circuit with a test lamp that is connected to a good ground. Refer to Probing Electrical Connectors .

Does the test lamp illuminate?

--

Go to Step 5

Go to Step 7

5 |

1. Turn OFF the ignition.
2. Jumper the CMP circuits from the CMP sensor to the CMP sensor harness connector. Refer to Using Connector Test Adapters .
3. Turn ON the ignition with the engine OFF.
4. Measure the Voltage Drop from the low reference circuit of the CMP sensor to a good ground with a DMM. Refer to Circuit Testing .

Is the voltage more than the specified value?

0.2 V

Go to Step 8

Go to Step 6

6 |

1. Leave the jumper wires installed.
2. Remove the jumper wire from the CMP signal circuit on the powertrain control module (PCM) side.
3. Start the engine.
4. Measure the duty cycle from the CMP signal circuit on the sensor side and to a good ground with a DMM.

Is the duty cycle within the specified range?

48-52%

Go to Step 9

Go to Step 10

7 | Test the 12-volt reference circuit for the following conditions:

• | An open

• | High resistance

• | A short to ground

Refer to Circuit Testing and Wiring Repairs .

Did you find and correct the condition?

--

Go to Step 15

Go to Step 11

8 | Test the low reference circuit for the following conditions:

• | An open

• | High resistance

Refer to Circuit Testing and Wiring Repairs .

Did you find and correct the condition?

--

Go to Step 15

Go to Step 11

9 | Test the signal circuit for the following conditions:

• | An open

• | A short to ground

• | A short to voltage

Refer to Circuit Testing and Wiring Repairs .

Did you find and correct the condition?

--

Go to Step 15

Go to Step 11

10 | Test for an intermittent and for a poor connection at the CMP sensor. Refer to Testing for Intermittent Conditions and Poor Connections and Connector Repairs . Did you find and correct the condition? | -- | Go to Step 15 | Go to Step 12
11 | Test for an intermittent and for a poor connection at the PCM. Refer to Testing for Intermittent Conditions and Poor Connections and Connector Repairs . Did you find and correct the condition? | -- | Go to Step 15 | Go to Step 14
12 |

1. Remove the CMP sensor.
2. Visually inspect the CMP sensor for the following conditions:

• | Physical damage

• | Loose or improper installation

Did you find and correct the condition?

--

Go to Step 15

Go to Step 13

13 | Replace the intake CMP sensor. Refer to Camshaft Position Sensor Replacement - Intake . Did you complete the replacement? | -- | Go to Step 15 | --
14 | Replace the PCM. Refer to Control Module References for replacement, setup, and programming. Did you complete the replacement? | -- | Go to Step 15 | --
15 |

1. Clear the DTCs with a scan tool.
2. Turn OFF the ignition for 30 seconds.
3. Start the engine.
4. Operate the vehicle within the Conditions for Running the DTC. You may also operate the vehicle within the conditions that you observed from the Freeze Frame/Failure Records.

Did the DTC fail this ignition?

--

Go to Step 2

Go to Step 16

16 | Observe the Capture Info with a scan tool. Are there any DTCs that have not been diagnosed? | -- | Go to Diagnostic Trouble Code (DTC) List - Vehicle | System OK