For 1990-2009 cars

### Removal Procedure

1. Open the console armrest, revealing the lower compartment.
2. Remove the 3 screws (1) located on the upper hinge.
3. Remove the armrest from the vehicle.

### Installation Procedure

1. Position the armrest to the console.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the 3 screws (1) retaining the armrest to the upper hinge.

Tighten
Tighten the screws to 1.5 N·m (15 lb in).

3. Close the armrest.