For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the nuts from the link assemblies.
3. Remove the link assemblies.
4. Inspect all of the parts for wear and damage.

### Installation Procedure

1. Support the lower control arms at curb height.
2. Install the link assemblies.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the nuts to the link assemblies.

Tighten
Tighten the nut to 44 N·m (32 lb ft).

4. Lower the vehicle.