For 1990-2009 cars

### Removal Procedure

1. Remove the front seat assembly. Refer to Front Seat Replacement - Bucket or Split Bench Seat Replacement .
2. Remove the front seat head restraint. Refer to Front Seat Head Restraint Replacement .
3. Pull the seat back cover and the seat back pad up high enough to expose the head restraint guides. Refer to Front Seat Back Cushion Cover and Cushion Pad Replacement .
4. Squeeze the retaining tabs located at the bottom of the guides together in order to remove the guides from the seat frame.
5. Remove the guides from the seat back frame.

### Installation Procedure

1. Install the guides to the seat back frame, verifying that the lower retainers are fully seated to the frame.
2. Install the guide with the locking tab (1) on the seat's right-hand side.
3. Install the seat back cover and pad. Refer to Front Seat Back Cushion Cover and Cushion Pad Replacement .
4. Install the front seat head restraint. Refer to Front Seat Head Restraint Replacement .
5. Install the seat assembly. Refer to Front Seat Replacement - Bucket or Split Bench Seat Replacement .