For 1990-2009 cars

## Seat Belt Replacement - Center Rear Crew Cab

### Removal Procedure

1. Remove the rear seat shoulder belt guide cover.
2. Remove the body rear trim panel. Refer to Body Rear Trim Panel Replacement.
3. Remove the bolt that retains the rear center seat belt assembly to the floor panel.
4. Remove the rear center seat belt assembly from the vehicle.

### Installation Procedure

1. Position the rear center seat belt assembly on the floor panel.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the bolt which retains the rear center seat belt assembly to the floor.

Tighten
Tighten the rear center seat belt bolt to 52.5 N·m (39 lb ft).

3. Route the rear center seat belt webbing up through the guide loop. Ensure that the seat belt webbing is not twisted.
4. Install the body rear trim panel. Refer to Body Rear Trim Panel Replacement.
5. Install the rear seat shoulder belt guide cover.